Castles Smart Card Development
============================================

    Header File - casmcard.h
    Library Name - libcasmcard.so
    Requirement - 
	Software : MUSCLE pcsc-lite components
        Driver : ez100pr.so v1.2.3 or higher (for EZ100PR Reader)
		 or
                 ez100pu.so v1.2.3 or higher (for EZ100PU Reader)
		 or
                 ezmini.so v1.2.3 or higher (for EZMINI Reader)
		 or
		 ez220pu.so v1.0.0 or higher (for EZ220PU Reader)
		or
		 ezusb.so v1.3.0 or higher (for EZ100PU/EZMINI/PISCES Reader)
    Version - 1.1.0
    Description - 
	1. Compatible with MUSCLE Smart Card Development (winscard.h)
	2. Allow to access memory card, i.e. SLE4442, SLE4428, SLE4404, SLE5536, I2C, etc.
    Installation - 
	1. Copy pcsclite libraries (libpcsclite.so, ....) to /lib. 
	   These libraries are usually located in /usr/local/lib after pcsclite installed.
	2. Copy libcasmcard.so to /lib.


    Simple Testing - 

	1. For SLE4428 - 
		In the example directory, run
			./rdrtest -h -m 0 1 3 
	2. For SLE4442 -         
		In the example directory, run
			./rdrtest -h -m 0 0 3 
   
